(module 208-8_CTSElectrocomponents (layer F.Cu) (tedit 5E2BCEA4)
  (descr "Dip Switch SPST 8 Position Through Hole Slide (Standard) Actuator 50mA 24VDC")
  (fp_text reference REF** (at 0 -6.35) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 208-8 (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -11.375 -5.015) (end -11.375 5.015) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.375 -5.015) (end 11.375 -5.015) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.375 5.015) (end 11.375 5.015) (layer F.SilkS) (width 0.12))
  (fp_line (start 11.375 -5.015) (end 11.375 5.015) (layer F.SilkS) (width 0.12))
  (pad 1 thru_hole roundrect (at -8.89 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad 2 thru_hole circle (at -6.35 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 6.35 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 8.89 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
)
