EESchema-DOCLIB  Version 2.0
#
$CMP 208-8_CTSElectrocomponents
D Dip Switch SPST 8 Position Through Hole Slide (Standard) Actuator 50mA 24VDC
F https://www.ctscorp.com/wp-content/uploads/208.pdf
$ENDCMP
#
$CMP DC10EWA_Kingbright
D LED Circuit Board Indicator Bar - 10 Wide, DIP Red (x 10) Diffused, White 2V 30mA  Through Hole
K LED BAR GRAPH 10SEG 627NM RED
F http://www.kingbrightusa.com/images/catalog/SPEC/DC10EWA.pdf
$ENDCMP
#
$CMP SN74HCT540N_TexasInstruments
D Buffer, Inverting 1 Element 8 Bit per Element 3-State Output 20-PDIP
F http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fsn74hct540
$ENDCMP
#
$CMP SN74HCT541N_TexasInstruments
D Buffer, Non-Inverting 1 Element 8 Bit per Element 3-State Output 20-PDIP
F http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fsn74hct541
$ENDCMP
#
#End Doc Library
