(module SS-13D16-VG_C&K (layer F.Cu) (tedit 5E2E44ED)
  (descr "Slide Switch SP3T Through Hole")
  (fp_text reference REF** (at 0 -3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SS-13D16-VG_C&K (at 0 -5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6.3 -2.15) (end 6.3 -2.15) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.3 2.15) (end 6.3 2.15) (layer F.SilkS) (width 0.12))
  (fp_line (start -6.3 -2.15) (end -6.3 2.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.3 -2.15) (end 6.3 2.15) (layer F.SilkS) (width 0.12))
  (pad 1 thru_hole roundrect (at -4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at -6.1 0) (size 2 2) (drill 1.25) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at 6.1 0) (size 2 2) (drill 1.25) (layers *.Cu *.Mask))
)
