(module G5V-2-DC3_OmronElectronics (layer F.Cu) (tedit 5E2E4218)
  (descr "General Purpose Relay DPDT (2 Form C) Through Hole")
  (fp_text reference REF** (at 0 -11.43) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value G5V-2-DC3_OmronElectronics (at 0 -13.97 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5.05 -10.25) (end -5.05 -10.25) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.05 10.25) (end 5.05 10.25) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.05 -10.25) (end 5.05 10.25) (layer F.SilkS) (width 0.12))
  (fp_line (start -5.05 -10.25) (end -5.05 10.25) (layer F.SilkS) (width 0.12))
  (pad 1 thru_hole roundrect (at -3.81 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  (pad 4 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at -3.81 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 3.81 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 3.81 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
)
