(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")

  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 152)
    (zones 0)
    (modules 13)
    (nets 36)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber & Drill/"))
  )

  (net 0 "")
  (net 1 "Net-(U1-Pad1)")
  (net 2 "Net-(U1-Pad2)")
  (net 3 "Net-(U1-Pad5)")
  (net 4 "Net-(U1-Pad3)")
  (net 5 "Net-(U1-Pad6)")
  (net 6 "Net-(U1-Pad8)")
  (net 7 "Net-(U1-Pad4)")
  (net 8 "Net-(U1-Pad7)")
  (net 9 GND)
  (net 10 "Net-(U4-Pad18)")
  (net 11 "Net-(U4-Pad17)")
  (net 12 "Net-(U4-Pad16)")
  (net 13 "Net-(U4-Pad15)")
  (net 14 "Net-(U4-Pad14)")
  (net 15 "Net-(U4-Pad13)")
  (net 16 "Net-(U4-Pad12)")
  (net 17 "Net-(U4-Pad11)")
  (net 18 VDC)
  (net 19 "Net-(U6-Pad20)")
  (net 20 "Net-(U6-Pad19)")
  (net 21 "Net-(U6-Pad2)")
  (net 22 "Net-(U6-Pad1)")
  (net 23 "Net-(U10-Pad2)")
  (net 24 "Net-(U13-Pad3)")
  (net 25 "Net-(U3-Pad2)")
  (net 26 "Net-(U11-Pad1)")
  (net 27 "Net-(U11-Pad2)")
  (net 28 "Net-(U11-Pad3)")
  (net 29 "Net-(U11-Pad4)")
  (net 30 "Net-(U11-Pad5)")
  (net 31 "Net-(U11-Pad6)")
  (net 32 "Net-(U11-Pad7)")
  (net 33 "Net-(U11-Pad8)")
  (net 34 "Net-(U10-Pad3)")
  (net 35 "Net-(U12-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U10-Pad3)")
    (add_net "Net-(U11-Pad1)")
    (add_net "Net-(U11-Pad2)")
    (add_net "Net-(U11-Pad3)")
    (add_net "Net-(U11-Pad4)")
    (add_net "Net-(U11-Pad5)")
    (add_net "Net-(U11-Pad6)")
    (add_net "Net-(U11-Pad7)")
    (add_net "Net-(U11-Pad8)")
    (add_net "Net-(U12-Pad1)")
    (add_net "Net-(U13-Pad3)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U4-Pad11)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad13)")
    (add_net "Net-(U4-Pad14)")
    (add_net "Net-(U4-Pad15)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad17)")
    (add_net "Net-(U4-Pad18)")
    (add_net "Net-(U6-Pad1)")
    (add_net "Net-(U6-Pad19)")
    (add_net "Net-(U6-Pad2)")
    (add_net "Net-(U6-Pad20)")
    (add_net VDC)
  )

  (module !Master:SS-13D16-VG_C&K (layer F.Cu) (tedit 5E2E44ED) (tstamp 5E3D2B33)
    (at 191.77 52.07)
    (descr "Slide Switch SP3T Through Hole")
    (path /5E3F1BC7)
    (fp_text reference U10 (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SS-13D16-VG_C&K (at 0 -16.51 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.3 -2.15) (end 6.3 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.3 -2.15) (end -6.3 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.3 2.15) (end 6.3 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.3 -2.15) (end 6.3 -2.15) (layer F.SilkS) (width 0.12))
    (pad "" thru_hole circle (at 6.1 0) (size 2 2) (drill 1.25) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -6.1 0) (size 2 2) (drill 1.25) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 3 thru_hole circle (at 2 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(U10-Pad3)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(U10-Pad2)"))
    (pad 1 thru_hole roundrect (at -4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 VDC))
  )

  (module !Master:DC10EWA_Kingbright (layer F.Cu) (tedit 5E2E4F39) (tstamp 5E3D2AFC)
    (at 175.26 63.5 270)
    (descr "LED Circuit Board Indicator Bar - 10 Wide, DIP Red (x 10) Diffused, White 2V 30mA  Through Hole")
    (path /5E2F2235)
    (fp_text reference U6 (at 0 1.27 270) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DC10EWA_Kingbright (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -12.7 4.08) (end -11.7 5.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -12.7 4.08) (end -12.7 -5.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.7 -5.08) (end -12.7 -5.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.7 5.08) (end 12.7 -5.08) (layer F.SilkS) (width 0.12))
    (fp_line (start -11.7 5.08) (end 12.7 5.08) (layer F.SilkS) (width 0.12))
    (pad 20 thru_hole circle (at -11.43 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(U6-Pad20)"))
    (pad 19 thru_hole circle (at -8.89 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(U6-Pad19)"))
    (pad 18 thru_hole circle (at -6.35 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "Net-(U11-Pad1)"))
    (pad 17 thru_hole circle (at -3.81 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(U11-Pad2)"))
    (pad 16 thru_hole circle (at -1.27 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(U11-Pad3)"))
    (pad 15 thru_hole circle (at 1.27 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(U11-Pad4)"))
    (pad 14 thru_hole circle (at 3.81 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(U11-Pad5)"))
    (pad 13 thru_hole circle (at 6.35 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(U11-Pad6)"))
    (pad 12 thru_hole circle (at 8.89 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(U11-Pad7)"))
    (pad 11 thru_hole circle (at 11.43 -3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(U11-Pad8)"))
    (pad 10 thru_hole circle (at 11.43 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(U4-Pad11)"))
    (pad 9 thru_hole circle (at 8.89 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(U4-Pad12)"))
    (pad 8 thru_hole circle (at 6.35 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(U4-Pad13)"))
    (pad 7 thru_hole circle (at 3.81 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(U4-Pad14)"))
    (pad 6 thru_hole circle (at 1.27 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U4-Pad15)"))
    (pad 5 thru_hole circle (at -1.27 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(U4-Pad16)"))
    (pad 4 thru_hole circle (at -3.81 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(U4-Pad17)"))
    (pad 3 thru_hole circle (at -6.35 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(U4-Pad18)"))
    (pad 2 thru_hole circle (at -8.89 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(U6-Pad2)"))
    (pad 1 thru_hole roundrect (at -11.43 3.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(U6-Pad1)"))
  )

  (module !Master:SS-13D16-VG_C&K (layer F.Cu) (tedit 5E2E44ED) (tstamp 5E3D2B71)
    (at 132.08 52.07)
    (descr "Slide Switch SP3T Through Hole")
    (path /5E307D84)
    (fp_text reference U13 (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SS-13D16-VG_C&K (at 0 -15.24 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.3 -2.15) (end 6.3 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.3 -2.15) (end -6.3 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.3 2.15) (end 6.3 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.3 -2.15) (end 6.3 -2.15) (layer F.SilkS) (width 0.12))
    (pad "" thru_hole circle (at 6.1 0) (size 2 2) (drill 1.25) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -6.1 0) (size 2 2) (drill 1.25) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 3 thru_hole circle (at 2 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(U13-Pad3)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(U12-Pad1)"))
    (pad 1 thru_hole roundrect (at -4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 VDC))
  )

  (module !Master:4116R-1-105LF_Bourns (layer F.Cu) (tedit 5E2E423A) (tstamp 5E3D2B63)
    (at 129.54 66.04)
    (descr "1M Ohm ±2% 250mW Power Per Element Isolated  Resistor Network/Array ±100ppm/°C 16-DIP (0.300\", 7.62mm)")
    (path /5E301913)
    (fp_text reference U12 (at 1.27 0 270) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4116R-1-105LF_Bourns (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.935 -10.985) (end 3.935 10.985) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.935 -10.985) (end -3.935 10.985) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.935 10.985) (end 3.935 10.985) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.935 -10.985) (end 3.935 -10.985) (layer F.SilkS) (width 0.12))
    (pad 16 thru_hole circle (at 3.81 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad1)"))
    (pad 15 thru_hole circle (at 3.81 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad2)"))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad3)"))
    (pad 13 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad4)"))
    (pad 12 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad5)"))
    (pad 11 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad6)"))
    (pad 10 thru_hole circle (at 3.81 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad7)"))
    (pad 9 thru_hole circle (at 3.81 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad8)"))
    (pad 8 thru_hole circle (at -3.81 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(U12-Pad1)"))
    (pad 7 thru_hole circle (at -3.81 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(U12-Pad1)"))
    (pad 6 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(U12-Pad1)"))
    (pad 5 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(U12-Pad1)"))
    (pad 4 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(U12-Pad1)"))
    (pad 3 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(U12-Pad1)"))
    (pad 2 thru_hole circle (at -3.81 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(U12-Pad1)"))
    (pad 1 thru_hole roundrect (at -3.81 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(U12-Pad1)"))
  )

  (module !Master:4116R-1-102LF_Bourns (layer F.Cu) (tedit 5E2E4249) (tstamp 5E3D2B4B)
    (at 194.31 66.04)
    (descr "1k Ohm ±2% 250mW Power Per Element Isolated  Resistor Network/Array ±100ppm/°C 16-DIP (0.300\", 7.62mm)")
    (path /5E451612)
    (fp_text reference U11 (at -1.27 0 270) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 4116R-1-102LF_Bourns (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.935 -10.985) (end 3.935 10.985) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.935 -10.985) (end -3.935 10.985) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.935 10.985) (end 3.935 10.985) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.935 -10.985) (end 3.935 -10.985) (layer F.SilkS) (width 0.12))
    (pad 16 thru_hole circle (at 3.81 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(U10-Pad2)"))
    (pad 15 thru_hole circle (at 3.81 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(U10-Pad2)"))
    (pad 14 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(U10-Pad2)"))
    (pad 13 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(U10-Pad2)"))
    (pad 12 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(U10-Pad2)"))
    (pad 11 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(U10-Pad2)"))
    (pad 10 thru_hole circle (at 3.81 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(U10-Pad2)"))
    (pad 9 thru_hole circle (at 3.81 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(U10-Pad2)"))
    (pad 8 thru_hole circle (at -3.81 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(U11-Pad8)"))
    (pad 7 thru_hole circle (at -3.81 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(U11-Pad7)"))
    (pad 6 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(U11-Pad6)"))
    (pad 5 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(U11-Pad5)"))
    (pad 4 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(U11-Pad4)"))
    (pad 3 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(U11-Pad3)"))
    (pad 2 thru_hole circle (at -3.81 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(U11-Pad2)"))
    (pad 1 thru_hole roundrect (at -3.81 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(U11-Pad1)"))
  )

  (module *Generic:8-PositionFemale_RectangularHeader (layer F.Cu) (tedit 5E3CD19F) (tstamp 5E3D2B26)
    (at 186.69 66.04)
    (path /5E48AF61)
    (fp_text reference U9 (at 0 -11.43) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 8-PositionFemale_RectangularHeader (at 0 -36.83 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 -10.16) (end -1.27 10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 10.16) (end 1.27 10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 10.16) (end 1.27 -10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 -10.16) (end -1.27 -10.16) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole roundrect (at 0 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(U11-Pad1)"))
    (pad 2 thru_hole circle (at 0 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(U11-Pad2)"))
    (pad 5 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(U11-Pad5)"))
    (pad 3 thru_hole circle (at 0 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(U11-Pad3)"))
    (pad 6 thru_hole circle (at 0 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(U11-Pad6)"))
    (pad 8 thru_hole circle (at 0 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(U11-Pad8)"))
    (pad 4 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(U11-Pad4)"))
    (pad 7 thru_hole circle (at 0 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(U11-Pad7)"))
  )

  (module *Generic:8-PositionMale_RectangularHeader (layer F.Cu) (tedit 5E3CD1B3) (tstamp 5E3D2B16)
    (at 184.15 66.04)
    (path /5E48A4A3)
    (fp_text reference U8 (at 0 -11.43) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 8-PositionMale_RectangularHeader (at 0 -35.56 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 -10.16) (end -1.27 -10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 10.16) (end 1.27 -10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 10.16) (end 1.27 10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -10.16) (end -1.27 10.16) (layer F.SilkS) (width 0.12))
    (pad 8 thru_hole circle (at 0 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(U11-Pad8)"))
    (pad 7 thru_hole circle (at 0 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(U11-Pad7)"))
    (pad 6 thru_hole circle (at 0 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(U11-Pad6)"))
    (pad 5 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(U11-Pad5)"))
    (pad 4 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(U11-Pad4)"))
    (pad 3 thru_hole circle (at 0 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(U11-Pad3)"))
    (pad 2 thru_hole circle (at 0 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(U11-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(U11-Pad1)"))
  )

  (module *Generic:2-PositionFemale_RectangularHeader (layer F.Cu) (tedit 5E3CD170) (tstamp 5E3D2B06)
    (at 162.56 52.07 90)
    (path /5E489277)
    (fp_text reference U7 (at 2.54 0 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2-PositionFemale_RectangularHeader (at 12.7 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 -2.54) (end -1.27 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 2.54) (end 1.27 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 2.54) (end 1.27 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -2.54) (end -1.27 2.54) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 0 1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole roundrect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 VDC))
  )

  (module *Generic:2-PositionMale_RectangularHeader (layer F.Cu) (tedit 5E3CD188) (tstamp 5E3D2ADF)
    (at 162.56 54.61 90)
    (path /5E507D51)
    (fp_text reference U5 (at -2.54 0 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2-PositionMale_RectangularHeader (at 12.7 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 -2.54) (end -1.27 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 2.54) (end 1.27 -2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 2.54) (end 1.27 2.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -2.54) (end -1.27 2.54) (layer F.SilkS) (width 0.12))
    (pad 2 thru_hole circle (at 0 1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 1 thru_hole roundrect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 VDC))
  )

  (module !Master:SN74HCT541N_TexasInstruments (layer F.Cu) (tedit 5E2E4F2E) (tstamp 5E3D2AD5)
    (at 149.86 63.5)
    (descr "Buffer, Inverting 1 Element 8 Bit per Element 3-State Output 20-PDIP")
    (path /5E2EEA39)
    (fp_text reference U4 (at -1.27 0 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SN74HCT541N_TexasInstruments (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.3 -13.46) (end 3.3 -13.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.3 13.46) (end 3.3 -13.46) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 13.46) (end 3.3 13.46) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.3 13.46) (end -3.3 -13.46) (layer F.SilkS) (width 0.12))
    (pad 20 thru_hole circle (at 3.81 -11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 VDC))
    (pad 19 thru_hole circle (at 3.81 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(U3-Pad2)"))
    (pad 18 thru_hole circle (at 3.81 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(U4-Pad18)"))
    (pad 17 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(U4-Pad17)"))
    (pad 9 thru_hole circle (at -3.81 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad8)"))
    (pad 10 thru_hole circle (at -3.81 11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad 11 thru_hole circle (at 3.81 11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(U4-Pad11)"))
    (pad 12 thru_hole circle (at 3.81 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(U4-Pad12)"))
    (pad 13 thru_hole circle (at 3.81 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(U4-Pad13)"))
    (pad 14 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(U4-Pad14)"))
    (pad 15 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U4-Pad15)"))
    (pad 16 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(U4-Pad16)"))
    (pad 1 thru_hole roundrect (at -3.81 -11.43) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(U3-Pad2)"))
    (pad 2 thru_hole circle (at -3.81 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad1)"))
    (pad 3 thru_hole circle (at -3.81 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad2)"))
    (pad 4 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad3)"))
    (pad 5 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad4)"))
    (pad 6 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad5)"))
    (pad 7 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad6)"))
    (pad 8 thru_hole circle (at -3.81 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad7)"))
  )

  (module !Master:OS102011MS2QN1_C&K (layer F.Cu) (tedit 5E2E46C6) (tstamp 5E3D2AB9)
    (at 162.56 74.93)
    (descr "Slide Switch SPDT Through Hole")
    (path /5E2ED8DF)
    (fp_text reference U3 (at 0 -3 180) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value OS102011MS2QN1_C&K (at 0 19.05 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -4.3 2.15) (end -4.3 -2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.3 2.15) (end 4.3 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.3 -2.15) (end 4.3 2.15) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.3 -2.15) (end 4.3 -2.15) (layer F.SilkS) (width 0.12))
    (pad 3 thru_hole circle (at 2 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 GND))
    (pad "" thru_hole circle (at -4.1 0) (size 2 2) (drill 1.25) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 4.1 0) (size 2 2) (drill 1.25) (layers *.Cu *.Mask))
    (pad 1 thru_hole roundrect (at -2 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 VDC))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(U3-Pad2)"))
  )

  (module *Generic:8-PositionMale_RectangularHeader (layer F.Cu) (tedit 5E3CD1B3) (tstamp 5E3D2AAC)
    (at 140.97 66.04)
    (path /5E48BF0A)
    (fp_text reference U2 (at 0 -11.43) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 8-PositionMale_RectangularHeader (at 0 -34.29 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 -10.16) (end -1.27 -10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 10.16) (end 1.27 -10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 10.16) (end 1.27 10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -10.16) (end -1.27 10.16) (layer F.SilkS) (width 0.12))
    (pad 8 thru_hole circle (at 0 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad8)"))
    (pad 7 thru_hole circle (at 0 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad7)"))
    (pad 6 thru_hole circle (at 0 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad6)"))
    (pad 5 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad5)"))
    (pad 4 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad4)"))
    (pad 3 thru_hole circle (at 0 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad3)"))
    (pad 2 thru_hole circle (at 0 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad1)"))
  )

  (module *Generic:8-PositionFemale_RectangularHeader (layer F.Cu) (tedit 5E3CD19F) (tstamp 5E3D2A9C)
    (at 138.43 66.04)
    (path /5E48C4EE)
    (fp_text reference U1 (at 0 -11.43) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 8-PositionFemale_RectangularHeader (at 0 -35.56 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 -10.16) (end -1.27 10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 10.16) (end 1.27 10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 10.16) (end 1.27 -10.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 -10.16) (end -1.27 -10.16) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole roundrect (at 0 -8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad2)"))
    (pad 5 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad5)"))
    (pad 3 thru_hole circle (at 0 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad3)"))
    (pad 6 thru_hole circle (at 0 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad6)"))
    (pad 8 thru_hole circle (at 0 8.89) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad8)"))
    (pad 4 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad4)"))
    (pad 7 thru_hole circle (at 0 6.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad7)"))
  )

  (gr_line (start 198.755 47.625) (end 201.93 50.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 201.93 76.2) (end 198.755 79.375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.095 79.375) (end 121.92 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.095 47.625) (end 121.92 50.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.92 76.2) (end 121.92 50.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 136.525 79.375) (end 125.095 79.375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.4 79.375) (end 136.525 79.375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.91 79.375) (end 152.4 79.375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 198.755 79.375) (end 168.91 79.375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 201.93 64.77) (end 201.93 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 201.93 50.8) (end 201.93 64.77) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.095 47.625) (end 198.755 47.625) (layer Edge.Cuts) (width 0.05))
  (gr_text "GND / NC / VDC" (at 132.08 48.895 180) (layer F.SilkS) (tstamp 5E3D1A9B)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "GND / NC / VDC" (at 191.77 48.895 180) (layer F.SilkS) (tstamp 5E3D1A96)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 2020-02-07-B (at 162.56 64.77 90) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text "Designed by\nWilliam Miceli" (at 175.26 63.5 90) (layer B.SilkS)
    (effects (font (size 2 2) (thickness 0.25)) (justify mirror))
  )
  (gr_text Power (at 162.56 49.53 180) (layer F.SilkS) (tstamp 5E3D5437)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text "Pull Resistors" (at 123.19 50.8 270) (layer F.SilkS) (tstamp 5E3D542F)
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
  )
  (gr_text "Output Connection" (at 200.66 50.8 90) (layer F.SilkS) (tstamp 5E3D542B)
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
  )
  (gr_text "Buffer Output" (at 162.56 78.105) (layer F.SilkS) (tstamp 5E3D53F0)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text Enable (at 164.465 71.755 90) (layer F.SilkS) (tstamp 5E3D53E1)
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
  )
  (gr_text Disable (at 160.655 71.755 90) (layer F.SilkS) (tstamp 5E3D53DA)
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
  )
  (gr_text GND (at 166.37 53.34 90) (layer F.SilkS) (tstamp 5E3D53D4)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text VDC (at 158.75 53.34 90) (layer F.SilkS) (tstamp 5E3D53CF)
    (effects (font (size 1 1) (thickness 0.15)))
  )

  (segment (start 140.97 57.15) (end 138.43 57.15) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 143.51 57.15) (end 146.05 54.61) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 140.97 57.15) (end 143.51 57.15) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 133.35 57.15) (end 138.43 57.15) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 138.43 59.69) (end 140.97 59.69) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 143.51 59.69) (end 146.05 57.15) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 140.97 59.69) (end 143.51 59.69) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 138.43 59.69) (end 133.35 59.69) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 140.97 67.31) (end 138.43 67.31) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 143.51 67.31) (end 146.05 64.77) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 140.97 67.31) (end 143.51 67.31) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 133.35 67.31) (end 138.43 67.31) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 140.97 62.23) (end 138.43 62.23) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 143.51 62.23) (end 146.05 59.69) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 140.97 62.23) (end 143.51 62.23) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 133.35 62.23) (end 138.43 62.23) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 138.43 69.85) (end 140.97 69.85) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 143.51 69.85) (end 146.05 67.31) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 140.97 69.85) (end 143.51 69.85) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 138.43 69.85) (end 133.35 69.85) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 138.43 74.93) (end 140.97 74.93) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 143.51 74.93) (end 146.05 72.39) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 140.97 74.93) (end 143.51 74.93) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 138.43 74.93) (end 133.35 74.93) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 138.43 64.77) (end 140.97 64.77) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 143.51 64.77) (end 146.05 62.23) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 140.97 64.77) (end 143.51 64.77) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 137.35237 64.77) (end 133.35 64.77) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 138.43 64.77) (end 137.35237 64.77) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 140.97 72.39) (end 138.43 72.39) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 143.51 72.39) (end 146.05 69.85) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 140.97 72.39) (end 143.51 72.39) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 133.35 72.39) (end 138.43 72.39) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 163.09763 77.47) (end 148.59 77.47) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 164.56 74.93) (end 164.56 76.00763) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 148.59 77.47) (end 146.05 74.93) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 164.56 76.00763) (end 163.09763 77.47) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 164.56 55.34) (end 163.83 54.61) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 164.56 74.93) (end 164.56 55.34) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 163.83 52.07) (end 163.83 54.61) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 195.77 50.99) (end 195.77 52.07) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 194.31 49.53) (end 195.77 50.99) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 166.37 49.53) (end 194.31 49.53) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 163.83 52.07) (end 163.83 50.8) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 163.83 50.8) (end 162.56 49.53) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 162.56 49.53) (end 140.335 49.53) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 140.335 49.53) (end 138.62 49.53) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 138.62 49.53) (end 137.795 49.53) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 136.08 52.07) (end 136.08 50.99) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 137.54 49.53) (end 137.795 49.53) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 136.08 50.99) (end 137.54 49.53) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 163.83 50.8) (end 165.1 49.53) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 165.1 49.53) (end 166.37 49.53) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 171.45 57.15) (end 153.67 57.15) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 171.45 59.69) (end 170.18 58.42) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 170.18 58.42) (end 154.94 58.42) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 154.94 58.42) (end 153.67 59.69) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 171.45 62.23) (end 168.91 59.69) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 168.91 59.69) (end 156.21 59.69) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 156.21 59.69) (end 153.67 62.23) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 171.45 64.77) (end 167.64 60.96) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 167.64 60.96) (end 157.48 60.96) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 157.48 60.96) (end 153.67 64.77) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 171.45 67.31) (end 166.37 62.23) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 166.37 62.23) (end 158.75 62.23) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 158.75 62.23) (end 153.67 67.31) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 171.45 69.85) (end 165.1 63.5) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 165.1 63.5) (end 160.02 63.5) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 160.02 63.5) (end 153.67 69.85) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 171.45 72.39) (end 163.83 64.77) (width 0.25) (layer F.Cu) (net 16))
  (segment (start 163.83 64.77) (end 161.29 64.77) (width 0.25) (layer F.Cu) (net 16))
  (segment (start 161.29 64.77) (end 153.67 72.39) (width 0.25) (layer F.Cu) (net 16))
  (segment (start 161.29 67.31) (end 163.83 67.31) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 161.29 67.31) (end 153.67 74.93) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 163.83 67.31) (end 171.45 74.93) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 160.56 55.34) (end 161.29 54.61) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 160.56 74.93) (end 160.56 55.34) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 161.29 52.07) (end 161.29 54.61) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 161.29 52.07) (end 153.67 52.07) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 161.29 52.07) (end 161.29 50.8) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 128.08 50.99) (end 128.08 52.07) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 129.54 49.53) (end 128.08 50.99) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 161.29 50.8) (end 160.02 49.53) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 160.02 49.53) (end 129.54 49.53) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 187.77 51.308) (end 187.77 52.07) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 185.992 49.53) (end 187.77 51.308) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 162.56 49.53) (end 185.992 49.53) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 161.29 50.8) (end 162.56 49.53) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 191.77 52.07) (end 191.77 53.975) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 194.945 57.15) (end 198.12 57.15) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 191.77 53.975) (end 194.945 57.15) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 198.12 57.15) (end 198.12 59.69) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 198.12 59.69) (end 198.12 62.23) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 198.12 64.77) (end 198.12 62.23) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 198.12 67.31) (end 198.12 64.77) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 198.12 68.77237) (end 198.12 67.31) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 198.12 69.85) (end 198.12 68.77237) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 198.12 72.39) (end 198.12 69.85) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 198.12 74.93) (end 198.12 72.39) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 145.288 52.07) (end 146.05 52.07) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 146.05 52.07) (end 148.59 52.07) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 151.13 54.61) (end 153.67 54.61) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 148.59 52.07) (end 151.13 54.61) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 153.67 54.61) (end 154.94 54.61) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 154.94 54.61) (end 156.21 55.88) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 162.56 73.66) (end 162.56 74.93) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 161.29 72.39) (end 162.56 73.66) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 158.75 72.39) (end 161.29 72.39) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 156.21 69.85) (end 158.75 72.39) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 156.21 55.88) (end 156.21 69.85) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 158.75 72.39) (end 158.75 72.39) (width 0.25) (layer B.Cu) (net 25) (tstamp 5E3D550D))
  (via (at 158.75 72.39) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 25))
  (segment (start 184.15 74.93) (end 186.69 74.93) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 184.15 72.39) (end 186.69 72.39) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 184.15 69.85) (end 186.69 69.85) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 184.15 67.31) (end 186.69 67.31) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 184.15 64.77) (end 186.69 64.77) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 184.15 62.23) (end 186.69 62.23) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 184.15 59.69) (end 186.69 59.69) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 184.15 57.15) (end 186.69 57.15) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 179.07 57.15) (end 184.15 57.15) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 189.738 57.15) (end 186.69 57.15) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 190.5 57.15) (end 189.738 57.15) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 184.15 59.69) (end 179.07 59.69) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 186.69 59.69) (end 190.5 59.69) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 179.07 62.23) (end 184.15 62.23) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 190.5 62.23) (end 186.69 62.23) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 183.07237 64.77) (end 179.07 64.77) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 184.15 64.77) (end 183.07237 64.77) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 187.76763 64.77) (end 190.5 64.77) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 186.69 64.77) (end 187.76763 64.77) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 179.07 67.31) (end 184.15 67.31) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 189.42237 67.31) (end 186.69 67.31) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 190.5 67.31) (end 189.42237 67.31) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 184.15 69.85) (end 179.07 69.85) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 186.69 69.85) (end 190.5 69.85) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 179.07 72.39) (end 184.15 72.39) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 189.42237 72.39) (end 186.69 72.39) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 190.5 72.39) (end 189.42237 72.39) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 184.15 74.93) (end 179.07 74.93) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 187.76763 74.93) (end 190.5 74.93) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 186.69 74.93) (end 187.76763 74.93) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 125.73 74.93) (end 125.73 72.39) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 125.73 69.85) (end 125.73 72.39) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 125.73 67.31) (end 125.73 69.85) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 125.73 64.77) (end 125.73 67.31) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 125.73 62.23) (end 125.73 64.77) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 125.73 59.69) (end 125.73 62.23) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 125.73 57.912) (end 125.73 59.69) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 125.73 57.15) (end 125.73 57.912) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 127 57.15) (end 125.73 57.15) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 132.08 52.07) (end 127 57.15) (width 0.25) (layer F.Cu) (net 35))

)
