@page hardware Hardware

@b Subpages

- @subpage designChoices
- @subpage deviceSpecifications

---



# Design Reminders

- From "Texas Instruments - SLAS655G...", Page 22:
  - To improve EMI on the XT1 oscillator, the following guidelines should be observed:
    - Keep the trace between the device and the crystal as short as possible.
    - Design a good ground plane around the oscillator pins.
    - Prevent crosstalk from other clock or data lines into oscillator pins XIN and XOUT.
    - Avoid running PCB traces underneath or adjacent to the XIN and XOUT pins.
