Inter-Integrated Circuit (I2C)=SDA,SCL
MCU_JTAG=TDO,TDI,TMS,TCK,R\S\T\,TEST,VCCTOOL
Serial Peripheral Interface (SPI)=C\S\,MOSI,MISO,SCLK
Universal Asynchronous Receiver-Transmitter (UART)=TX,RX
Vehicle Lighting - Braking=0,1,2,3,4
Vehicle Lighting - Daytime Running=0,1,2,3
Vehicle Lighting - Left Indicators=0,1,2,3
Vehicle Lighting - Right Indicators=0,1,2,3
