\let\mypdfximage\pdfximage\def\pdfximage{\immediate\mypdfximage}\documentclass[twoside]{book}

%% moved from doxygen.sty due to workaround for LaTex 2019 version and unmaintained tabu package
\usepackage{ifthen}
\ifx\requestedLaTeXdate\undefined
\usepackage{array}
\else
\usepackage{array}[=2016-10-06]
\fi
%%
% Packages required by doxygen
\usepackage{fixltx2e}
\usepackage{doxygen}
\usepackage{graphicx}
\usepackage[utf8]{inputenc}
\usepackage{makeidx}
\PassOptionsToPackage{warn}{textcomp}
\usepackage{textcomp}
\usepackage[nointegrals]{wasysym}
\usepackage{ifxetex}

% Font selection
\usepackage[T1]{fontenc}
\usepackage[scaled=.90]{helvet}
\usepackage{courier}
\renewcommand{\familydefault}{\sfdefault}
\usepackage{sectsty}
\allsectionsfont{%
  \fontseries{bc}\selectfont%
  \color{darkgray}%
}
\renewcommand{\DoxyLabelFont}{%
  \fontseries{bc}\selectfont%
  \color{darkgray}%
}
\newcommand{\+}{\discretionary{\mbox{\scriptsize$\hookleftarrow$}}{}{}}

% Arguments of doxygenemoji:
% 1) ':<text>:' form of the emoji, already "LaTeX"-escaped
% 2) file with the name of the emoji without the .png extension
% in case image exist use this otherwise use the ':<text>:' form
\newcommand{\doxygenemoji}[2]{%
  \IfFileExists{./#2.png}{\raisebox{-0.1em}{\includegraphics[height=0.9em]{./#2.png}}}{#1}%
}
% Page & text layout
\usepackage{geometry}
\geometry{%
  a4paper,%
  top=2.5cm,%
  bottom=2.5cm,%
  left=2.5cm,%
  right=2.5cm%
}
\tolerance=750
\hfuzz=15pt
\hbadness=750
\setlength{\emergencystretch}{15pt}
\setlength{\parindent}{0cm}
\newcommand{\doxynormalparskip}{\setlength{\parskip}{3ex plus 2ex minus 2ex}}
\newcommand{\doxytocparskip}{\setlength{\parskip}{1ex plus 0ex minus 0ex}}
\doxynormalparskip
\makeatletter
\renewcommand{\paragraph}{%
  \@startsection{paragraph}{4}{0ex}{-1.0ex}{1.0ex}{%
    \normalfont\normalsize\bfseries\SS@parafont%
  }%
}
\renewcommand{\subparagraph}{%
  \@startsection{subparagraph}{5}{0ex}{-1.0ex}{1.0ex}{%
    \normalfont\normalsize\bfseries\SS@subparafont%
  }%
}
\makeatother

\makeatletter
\newcommand\hrulefilll{\leavevmode\leaders\hrule\hskip 0pt plus 1filll\kern\z@}
\makeatother

% Headers & footers
\usepackage{fancyhdr}
\pagestyle{fancyplain}
\renewcommand{\footrulewidth}{0.4pt}
%
\fancypagestyle{fancyplain}{
\fancyhf{}
\fancyhead[LE, RO]{\bfseries\thepage}
\fancyhead[LO]{\bfseries\rightmark}
\fancyhead[RE]{\bfseries\leftmark}
\fancyfoot[LO, RE]{\bfseries\scriptsize Generated by Doxygen }
}
%
\fancypagestyle{plain}{
\fancyhf{}
\fancyfoot[LO, RE]{\bfseries\scriptsize Generated by Doxygen }
\renewcommand{\headrulewidth}{0pt}}
%
\pagestyle{fancyplain}
%
\renewcommand{\chaptermark}[1]{%
  \markboth{#1}{}%
}
\renewcommand{\sectionmark}[1]{%
  \markright{\thesection\ #1}%
}

% Indices & bibliography
\usepackage{natbib}
\usepackage[titles]{tocloft}
\setcounter{tocdepth}{3}
\setcounter{secnumdepth}{5}
\makeindex

\usepackage{newunicodechar}
  \newunicodechar{⁻}{${}^{-}$}% Superscript minus
  \newunicodechar{²}{${}^{2}$}% Superscript two
  \newunicodechar{³}{${}^{3}$}% Superscript three

% Hyperlinks (required, but should be loaded last)
\ifpdf
  \usepackage[pdftex,pagebackref=true]{hyperref}
\else
  \ifxetex
    \usepackage[pagebackref=true]{hyperref}
  \else
    \usepackage[ps2pdf,pagebackref=true]{hyperref}
  \fi
\fi

\hypersetup{%
  colorlinks=true,%
  linkcolor=blue,%
  citecolor=blue,%
  unicode%
}

% Custom commands
\newcommand{\clearemptydoublepage}{%
  \newpage{\pagestyle{empty}\cleardoublepage}%
}

\usepackage{caption}
\captionsetup{labelsep=space,justification=centering,font={bf},singlelinecheck=off,skip=4pt,position=top}

\usepackage{etoc}
\etocsettocstyle{\doxytocparskip}{\doxynormalparskip}
\renewcommand{\numberline}[1]{#1~}
%===== C O N T E N T S =====

\begin{document}
\raggedbottom

% Titlepage & ToC
\hypersetup{pageanchor=false,
             bookmarksnumbered=true,
             pdfencoding=unicode
            }
\pagenumbering{alph}
\begin{titlepage}
\vspace*{7cm}
\begin{center}%
{\Large 2020-\/2021 Sunseeker Telemetry and Lighting System }\\
\vspace*{1cm}
{\large Generated by Doxygen 1.9.1}\\
\end{center}
\end{titlepage}
\clearemptydoublepage
\pagenumbering{roman}
\tableofcontents
\clearemptydoublepage
\pagenumbering{arabic}
\hypersetup{pageanchor=true}

%--- Begin generated contents ---
\chapter{Home}
\label{index}\hypertarget{index}{}\input{index}
\chapter{Hardware}
\label{hardware}
\Hypertarget{hardware}
\input{hardware}
\chapter{Software}
\label{software}
\Hypertarget{software}
\input{software}
\chapter{Documentation Guide}
\label{documentation_guide}
\Hypertarget{documentation_guide}
\input{documentation_guide}
\chapter{Resources}
\label{resources}
\Hypertarget{resources}
\input{resources}
\chapter{Module Index}
\input{modules}
\chapter{Namespace Index}
\input{namespaces}
\chapter{Data Structure Index}
\input{annotated}
\chapter{File Index}
\input{files}
\chapter{Module Documentation}
\input{group__adc10__a__api}
\input{group__adc12__a__api}
\input{group__aes__api}
\input{group__battbak__api}
\input{group__comp__b__api}
\input{group__crc__api}
\input{group__ctsd16__api}
\input{group__dac12__a__api}
\input{group__dma__api}
\input{group__eusci__a__spi__api}
\input{group__eusci__a__uart__api}
\input{group__eusci__b__i2c__api}
\input{group__eusci__b__spi__api}
\input{group__flashctl__api}
\input{group__gpio__api}
\input{group__lcd__b__api}
\input{group__lcd__c__api}
\input{group__ldopwr__api}
\input{group__mpy32__api}
\input{group__oa__api}
\input{group__pmap__api}
\input{group__pmm__api}
\input{group__ram__api}
\input{group__ref__api}
\input{group__rtc__a__api}
\input{group__rtc__b__api}
\input{group__rtc__c__api}
\input{group__sd24__b__api}
\input{group__sfr__api}
\input{group__sysctl__api}
\input{group__tec__api}
\input{group__timer__a__api}
\input{group__timer__b__api}
\input{group__timer__d__api}
\input{group__tlv__api}
\input{group__ucs__api}
\input{group__usci__a__spi__api}
\input{group__usci__a__uart__api}
\input{group__usci__b__i2c__api}
\input{group__usci__b__spi__api}
\input{group__wdt__a__api}
\input{group__dac12__examples__list}
\input{group__ref__examples__list}
\chapter{Namespace Documentation}
\input{namespacelextab}
\input{namespaceyacctab}
\chapter{Data Structure Documentation}
\input{classti__mcu__msp430__driverlib__product}
\chapter{File Documentation}
\input{_9_hardware_8markdown}
\input{_design_01_choices_8markdown}
\input{_device_01_specifications_8markdown}
\input{_power_01_design_8markdown}
\input{_documentation_01_guide_8markdown}
\input{_r_e_a_d_m_e_8markdown}
\input{_9_resources_8markdown}
\input{adc10__a__ex1__avcc_ref_8c}
\input{adc10__a__ex2__int_ref_8c}
\input{adc10__a__ex3__window_comp_8c}
\input{adc10__a__ex4__signed_data_8c}
\input{adc10__a__ex5__batt_monitor_8c}
\input{adc10__a__ex6__ref_toggle_8c}
\input{adc10__a__ex7__repeat_single_d_m_a_8c}
\input{adc10__a__ex8__sequence_d_m_a_8c}
\input{adc10__a__ex9__repeat_seq_8c}
\input{adc12__a__ex1__avcc_ref_8c}
\input{adc12__a__ex2__int_ref_8c}
\input{adc12__a__ex3__ext_ref_8c}
\input{adc12__a__ex4__repeated_seq_8c}
\input{adc12__a__ex5__repeated_single_8c}
\input{adc12__a__ex6__extended_inputs_8c}
\input{adc12__a__ex7__sequence_8c}
\input{adc12__a__ex8__temp_sensor_8c}
\input{aes__ex1__encrypt_decrypt_8c}
\input{aes__ex2__encrypt_decrypt_with_first_round_key_8c}
\input{battbak__ex1__calendermode_l_p_m3_8c}
\input{comp__b__ex1__2_v_ref_8c}
\input{comp__b__ex2__1_v5_ref_int_8c}
\input{comp__b__ex3__avcc_ref_u_l_p_m_8c}
\input{comp__b__ex4__hysteresis_8c}
\input{comp__b__ex5___t_ax_8c}
\input{comp__b__ex6__ext_ref_8c}
\input{_m_s_p430_f5xx__6xx_2crc_2crc__ex1__build_signature_8c}
\input{_m_s_p430_f_r2xx__4xx_2crc_2crc__ex1__build_signature_8c}
\input{_m_s_p430_f_r57xx_2crc_2crc__ex1__build_signature_8c}
\input{_m_s_p430_f_r5xx__6xx_2crc_2crc__ex1__build_signature_8c}
\input{ctsd16__ex1__single_ch_cont_conv_8c}
\input{ctsd16__ex2__single_ch_single_conv_polling_8c}
\input{ctsd16__ex3__single_ch_single_conv_interrupt_8c}
\input{ctsd16__ex4__internal_temp_sensor_8c}
\input{ctsd16__ex5__three_ch_single_conv_8c}
\input{dac12__a__ex1__1_v5_out_8c}
\input{dac12__a__ex2__0_v75_out_8c}
\input{dac12__a__ex3__positive_ramp_int_8c}
\input{dac12__a__ex4__grouped_8c}
\input{_m_s_p430_f5xx__6xx_2dma_2dma__ex1__repeated_block_8c}
\input{_m_s_p430_f_r57xx_2dma_2dma__ex1__repeated_block_8c}
\input{_m_s_p430_f_r5xx__6xx_2dma_2dma__ex1__repeated_block_8c}
\input{dma__ex2__repeated_block_u_a_r_t_8c}
\input{dma__ex3__single_transfer_s_p_i_8c}
\input{dma__ex4__single_transfer_a_d_c12_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__a__spi_2eusci__a__spi__ex1__master_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__a__spi_2eusci__a__spi__ex1__master_8c}
\input{_m_s_p430_f_r57xx_2eusci__a__spi_2eusci__a__spi__ex1__master_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__a__spi_2eusci__a__spi__ex1__master_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__a__spi_2eusci__a__spi__ex1__slave_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__a__spi_2eusci__a__spi__ex1__slave_8c}
\input{_m_s_p430_f_r57xx_2eusci__a__spi_2eusci__a__spi__ex1__slave_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__a__spi_2eusci__a__spi__ex1__slave_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__a__uart_2eusci__a__uart__ex1__loopback_advanced_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__a__uart_2eusci__a__uart__ex1__loopback_advanced_8c}
\input{_m_s_p430_f_r57xx_2eusci__a__uart_2eusci__a__uart__ex1__loopback_advanced_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__a__uart_2eusci__a__uart__ex1__loopback_advanced_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex1__master_rx_multiple_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__i2c_2eusci__b__i2c__ex1__master_rx_multiple_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__i2c_2eusci__b__i2c__ex1__master_rx_multiple_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex1__master_rx_multiple_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex1__slave_tx_multiple_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__i2c_2eusci__b__i2c__ex1__slave_tx_multiple_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__i2c_2eusci__b__i2c__ex1__slave_tx_multiple_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex1__slave_tx_multiple_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex2__master_rx_single_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__i2c_2eusci__b__i2c__ex2__master_rx_single_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__i2c_2eusci__b__i2c__ex2__master_rx_single_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex2__master_rx_single_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex2__slave_tx_single_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__i2c_2eusci__b__i2c__ex2__slave_tx_single_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__i2c_2eusci__b__i2c__ex2__slave_tx_single_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex2__slave_tx_single_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex3__master_tx_multiple_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__i2c_2eusci__b__i2c__ex3__master_tx_multiple_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__i2c_2eusci__b__i2c__ex3__master_tx_multiple_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex3__master_tx_multiple_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex3__slave_rx_multiple_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__i2c_2eusci__b__i2c__ex3__slave_rx_multiple_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__i2c_2eusci__b__i2c__ex3__slave_rx_multiple_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex3__slave_rx_multiple_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex4__master_tx_single_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__i2c_2eusci__b__i2c__ex4__master_tx_single_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__i2c_2eusci__b__i2c__ex4__master_tx_single_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex4__master_tx_single_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex4__slave_rx_single_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__i2c_2eusci__b__i2c__ex4__slave_rx_single_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__i2c_2eusci__b__i2c__ex4__slave_rx_single_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex4__slave_rx_single_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex5__master_multiple_slave_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__i2c_2eusci__b__i2c__ex5__master_multiple_slave_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__i2c_2eusci__b__i2c__ex5__master_multiple_slave_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex5__master_multiple_slave_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex5__slave_multiple_slave_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__i2c_2eusci__b__i2c__ex5__slave_multiple_slave_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__i2c_2eusci__b__i2c__ex5__slave_multiple_slave_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__i2c_2eusci__b__i2c__ex5__slave_multiple_slave_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__spi_2eusci__b__spi__ex1__master_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__spi_2eusci__b__spi__ex1__master_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__spi_2eusci__b__spi__ex1__master_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__spi_2eusci__b__spi__ex1__master_8c}
\input{_m_s_p430_f5xx__6xx_2eusci__b__spi_2eusci__b__spi__ex1__slave_8c}
\input{_m_s_p430_f_r2xx__4xx_2eusci__b__spi_2eusci__b__spi__ex1__slave_8c}
\input{_m_s_p430_f_r57xx_2eusci__b__spi_2eusci__b__spi__ex1__slave_8c}
\input{_m_s_p430_f_r5xx__6xx_2eusci__b__spi_2eusci__b__spi__ex1__slave_8c}
\input{flashctl__ex1__write_to_info_b_8c}
\input{flashctl__ex2__erase_copy_write_8c}
\input{flashctl__ex3__long_word_write_8c}
\input{flashctl__ex4__write_to_info_a_8c}
\input{_m_s_p430_f5xx__6xx_2gpio_2gpio__ex1__output_hi_8c}
\input{_m_s_p430_f_r2xx__4xx_2gpio_2gpio__ex1__output_hi_8c}
\input{_m_s_p430_f_r57xx_2gpio_2gpio__ex1__output_hi_8c}
\input{_m_s_p430_f_r5xx__6xx_2gpio_2gpio__ex1__output_hi_8c}
\input{_m_s_p430_f5xx__6xx_2gpio_2gpio__ex2__input_capture_8c}
\input{_m_s_p430_f_r2xx__4xx_2gpio_2gpio__ex2__input_capture_8c}
\input{_m_s_p430_f_r57xx_2gpio_2gpio__ex2__input_capture_8c}
\input{_m_s_p430_f_r5xx__6xx_2gpio_2gpio__ex2__input_capture_8c}
\input{_m_s_p430_f5xx__6xx_2gpio_2gpio__ex3__software_poll_8c}
\input{_m_s_p430_f_r2xx__4xx_2gpio_2gpio__ex3__software_poll_8c}
\input{_m_s_p430_f_r57xx_2gpio_2gpio__ex3__software_poll_8c}
\input{_m_s_p430_f_r5xx__6xx_2gpio_2gpio__ex3__software_poll_8c}
\input{_m_s_p430_f5xx__6xx_2gpio_2gpio__ex4__write_to_port1_8c}
\input{_m_s_p430_f_r2xx__4xx_2gpio_2gpio__ex4__write_to_port1_8c}
\input{_m_s_p430_f_r57xx_2gpio_2gpio__ex4__write_to_port1_8c}
\input{_m_s_p430_f_r5xx__6xx_2gpio_2gpio__ex4__write_to_port1_8c}
\input{lcd__b__ex1__4mux_8c}
\input{ldopwr__ex1__internal_l_d_o_power_8c}
\input{ldopwr__ex2__software_poll_8c}
\input{ldopwr__ex3__internal_l_d_o_enabled_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex10__32bit_signed_multiply_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex10__32bit_signed_multiply_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex10__32bit_signed_multiply_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex10__32bit_signed_multiply_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex11__32bit_signed_multiply_accum_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex11__32bit_signed_multiply_accum_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex11__32bit_signed_multiply_accum_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex11__32bit_signed_multiply_accum_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex12__32bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex12__32bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex12__32bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex12__32bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex13__saturation_underflow_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex13__saturation_underflow_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex13__saturation_underflow_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex13__saturation_underflow_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex14__saturation_overflow_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex14__saturation_overflow_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex14__saturation_overflow_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex14__saturation_overflow_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex15__fraction_mode_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex15__fraction_mode_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex15__fraction_mode_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex15__fraction_mode_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex1__16bit_unsigned_multiply_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex1__16bit_unsigned_multiply_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex1__16bit_unsigned_multiply_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex1__16bit_unsigned_multiply_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex2__8bit_unsigned_multiply_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex2__8bit_unsigned_multiply_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex2__8bit_unsigned_multiply_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex2__8bit_unsigned_multiply_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex3__16bit_signed_multiply_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex3__16bit_signed_multiply_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex3__16bit_signed_multiply_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex3__16bit_signed_multiply_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex4__8bit_signed_multiply_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex4__8bit_signed_multiply_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex4__8bit_signed_multiply_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex4__8bit_signed_multiply_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex5__16bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex5__16bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex5__16bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex5__16bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex6__8bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex6__8bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex6__8bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex6__8bit_unsigned_multiply_accum_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex7__16bit_signed_multiply_accum_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex7__16bit_signed_multiply_accum_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex7__16bit_signed_multiply_accum_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex7__16bit_signed_multiply_accum_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex8__8bit_signed_multiply_accum_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex8__8bit_signed_multiply_accum_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex8__8bit_signed_multiply_accum_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex8__8bit_signed_multiply_accum_8c}
\input{_m_s_p430_f5xx__6xx_2mpy32_2mpy32__ex9__32bit_unsigned_multiply_8c}
\input{_m_s_p430_f_r2xx__4xx_2mpy32_2mpy32__ex9__32bit_unsigned_multiply_8c}
\input{_m_s_p430_f_r57xx_2mpy32_2mpy32__ex9__32bit_unsigned_multiply_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpy32_2mpy32__ex9__32bit_unsigned_multiply_8c}
\input{oa__ex1__general_purpose_8c}
\input{oa__ex2__general_purpose_8c}
\input{oa__ex3__unity_gain_buffer_8c}
\input{pmap__ex1__single_runtime_config_8c}
\input{pmap__ex2__output_timer_b_signal_8c}
\input{pmap__ex3__single_function_to_multiple_pins_8c}
\input{pmm__ex1__vcore3_8c}
\input{pmm__ex2__fast_wake_up_8c}
\input{pmm__ex3__low_current_consumption_8c}
\input{ram__ex1__turn_off_sector_8c}
\input{ref__ex1___a_d_c12_ctl_8c}
\input{rtc__a__ex1__calendermode_8c}
\input{rtc__a__ex2__countermode_8c}
\input{rtc__b__ex1__calendermode_l_p_m0_8c}
\input{rtc__b__ex2__calendermode_l_p_m3_8c}
\input{_m_s_p430_f5xx__6xx_2rtc__c_2rtc__c__ex1__calendarmode_8c}
\input{_m_s_p430_f_r5xx__6xx_2rtc__c_2rtc__c__ex1__calendarmode_8c}
\input{sd24__b__ex1__single_conv_single_channel_8c}
\input{sd24__b__ex2__single_conv_channel_group_8c}
\input{sd24__b__ex3__cont_conv_single_channel_8c}
\input{tec__ex1__sync_timers_8c}
\input{tec__ex2__ext_clear_input_8c}
\input{_m_s_p430_f5xx__6xx_2timer__a_2timer__a__ex1__pwm_single_8c}
\input{_m_s_p430_f_r2xx__4xx_2timer__a_2timer__a__ex1__pwm_single_8c}
\input{_m_s_p430_f_r57xx_2timer__a_2timer__a__ex1__pwm_single_8c}
\input{_m_s_p430_f_r5xx__6xx_2timer__a_2timer__a__ex1__pwm_single_8c}
\input{_m_s_p430_f5xx__6xx_2timer__a_2timer__a__ex2__continous_mode_operation_with_c_c_r0_interrupt_8c}
\input{_m_s_p430_f_r2xx__4xx_2timer__a_2timer__a__ex2__continous_mode_operation_with_c_c_r0_interrupt_8c}
\input{_m_s_p430_f_r57xx_2timer__a_2timer__a__ex2__continous_mode_operation_with_c_c_r0_interrupt_8c}
\input{_m_s_p430_f_r5xx__6xx_2timer__a_2timer__a__ex2__continous_mode_operation_with_c_c_r0_interrupt_8c}
\input{_m_s_p430_f5xx__6xx_2timer__a_2timer__a__ex3__continous_mode_operation_with_t_a_i_e_interrupt_8c}
\input{_m_s_p430_f_r2xx__4xx_2timer__a_2timer__a__ex3__continous_mode_operation_with_t_a_i_e_interrupt_8c}
\input{_m_s_p430_f_r57xx_2timer__a_2timer__a__ex3__continous_mode_operation_with_t_a_i_e_interrupt_8c}
\input{_m_s_p430_f_r5xx__6xx_2timer__a_2timer__a__ex3__continous_mode_operation_with_t_a_i_e_interrupt_8c}
\input{_m_s_p430_f5xx__6xx_2timer__a_2timer__a__ex4__pwm_multiple_up_down_8c}
\input{_m_s_p430_f_r2xx__4xx_2timer__a_2timer__a__ex4__pwm_multiple_up_down_8c}
\input{_m_s_p430_f_r57xx_2timer__a_2timer__a__ex4__pwm_multiple_up_down_8c}
\input{_m_s_p430_f_r5xx__6xx_2timer__a_2timer__a__ex4__pwm_multiple_up_down_8c}
\input{_m_s_p430_f5xx__6xx_2timer__a_2timer__a__ex5__pwm_multiple_up_8c}
\input{_m_s_p430_f_r2xx__4xx_2timer__a_2timer__a__ex5__pwm_multiple_up_8c}
\input{_m_s_p430_f_r57xx_2timer__a_2timer__a__ex5__pwm_multiple_up_8c}
\input{_m_s_p430_f_r5xx__6xx_2timer__a_2timer__a__ex5__pwm_multiple_up_8c}
\input{_m_s_p430_f5xx__6xx_2timer__a_2timer__a__ex6__up_down_mode_operation_8c}
\input{_m_s_p430_f_r2xx__4xx_2timer__a_2timer__a__ex6__up_down_mode_operation_8c}
\input{_m_s_p430_f_r57xx_2timer__a_2timer__a__ex6__up_down_mode_operation_8c}
\input{_m_s_p430_f_r5xx__6xx_2timer__a_2timer__a__ex6__up_down_mode_operation_8c}
\input{_m_s_p430_f5xx__6xx_2timer__b_2timer__b__ex1__continuous_mode_c_c_r0_8c}
\input{_m_s_p430_f_r2xx__4xx_2timer__b_2timer__b__ex1__continuous_mode_c_c_r0_8c}
\input{_m_s_p430_f_r57xx_2timer__b_2timer__b__ex1__continuous_mode_c_c_r0_8c}
\input{_m_s_p430_f_r5xx__6xx_2timer__b_2timer__b__ex1__continuous_mode_c_c_r0_8c}
\input{_m_s_p430_f5xx__6xx_2timer__b_2timer__b__ex2__overflow_i_s_r_8c}
\input{_m_s_p430_f_r2xx__4xx_2timer__b_2timer__b__ex2__overflow_i_s_r_8c}
\input{_m_s_p430_f_r57xx_2timer__b_2timer__b__ex2__overflow_i_s_r_8c}
\input{_m_s_p430_f_r5xx__6xx_2timer__b_2timer__b__ex2__overflow_i_s_r_8c}
\input{_m_s_p430_f5xx__6xx_2timer__b_2timer__b__ex3__pwm_8c}
\input{_m_s_p430_f_r2xx__4xx_2timer__b_2timer__b__ex3__pwm_8c}
\input{_m_s_p430_f_r57xx_2timer__b_2timer__b__ex3__pwm_8c}
\input{_m_s_p430_f_r5xx__6xx_2timer__b_2timer__b__ex3__pwm_8c}
\input{_m_s_p430_f5xx__6xx_2timer__b_2timer__b__ex4__up_mode_operation_8c}
\input{_m_s_p430_f_r2xx__4xx_2timer__b_2timer__b__ex4__up_mode_operation_8c}
\input{_m_s_p430_f_r57xx_2timer__b_2timer__b__ex4__up_mode_operation_8c}
\input{_m_s_p430_f_r5xx__6xx_2timer__b_2timer__b__ex4__up_mode_operation_8c}
\input{_m_s_p430_f5xx__6xx_2timer__b_2timer__b__ex5__single_p_w_m_8c}
\input{_m_s_p430_f_r2xx__4xx_2timer__b_2timer__b__ex5__single_p_w_m_8c}
\input{_m_s_p430_f_r57xx_2timer__b_2timer__b__ex5__single_p_w_m_8c}
\input{_m_s_p430_f_r5xx__6xx_2timer__b_2timer__b__ex5__single_p_w_m_8c}
\input{timer__d__ex10__duty_cycle_measurement_dual_8c}
\input{timer__d__ex1__cont_c_r_r0_8c}
\input{timer__d__ex2__overflow_i_s_r_8c}
\input{timer__d__ex3__up_down_mode_8c}
\input{timer__d__ex4__pwm_up_down_mode_8c}
\input{timer__d__ex5__hi_res_free_running_p_w_m_8c}
\input{timer__d__ex6__hi_res_regulated_p_w_m_8c}
\input{timer__d__ex7__combine_regs_p_w_m_8c}
\input{timer__d__ex8__duty_cycle_measurement_single_8c}
\input{timer__d__ex9__period_measurement_8c}
\input{_m_s_p430_f5xx__6xx_2tlv_2tlv__ex1__get_device_type_8c}
\input{_m_s_p430_f_r2xx__4xx_2tlv_2tlv__ex1__get_device_type_8c}
\input{_m_s_p430_f_r57xx_2tlv_2tlv__ex1__get_device_type_8c}
\input{_m_s_p430_f_r5xx__6xx_2tlv_2tlv__ex1__get_device_type_8c}
\input{_m_s_p430_f5xx__6xx_2tlv_2tlv__ex2__read_t_l_v_descriptors_8c}
\input{_m_s_p430_f_r5xx__6xx_2tlv_2tlv__ex2__read_t_l_v_descriptors_8c}
\input{_m_s_p430_f5xx__6xx_2tlv_2tlv__ex3__calibrate_temp_sensor_8c}
\input{_m_s_p430_f_r5xx__6xx_2tlv_2tlv__ex3__calibrate_temp_sensor_8c}
\input{ucs__ex1___d_c_o12_m_hz_8c}
\input{ucs__ex2___v_l_o_sources_a_c_l_k_8c}
\input{ucs__ex3___x_t1_sources_a_c_l_k_8c}
\input{ucs__ex4___x_t_sources_d_c_o_internal_8c}
\input{usci__a__spi__ex1__master_8c}
\input{usci__a__spi__ex1__slave_8c}
\input{usci__a__uart__ex1__loopback_advance_8c}
\input{usci__a__uart__ex2__address_bit_multiprocessor_r_x_8c}
\input{usci__a__uart__ex2__address_bit_multiprocessor_t_x_8c}
\input{usci__a__uart__ex3__auto_baudrate_detection_r_x_8c}
\input{usci__a__uart__ex3__auto_baudrate_detection_t_x_8c}
\input{usci__a__uart__ex4__idle_line_multiprocessor_r_x_8c}
\input{usci__a__uart__ex4__idleline_multiprocessor_t_x_8c}
\input{usci__b__i2c__ex1__master_rx_single_8c}
\input{usci__b__i2c__ex1__slave_tx_single_8c}
\input{usci__b__i2c__ex2__master_tx_multiple_8c}
\input{usci__b__i2c__ex2__slave_rx_multiple_8c}
\input{usci__b__i2c__ex3__master_tx_single_8c}
\input{usci__b__i2c__ex3__slave_rx_single_8c}
\input{usci__b__i2c__ex4__master_rx_multiple_8c}
\input{usci__b__i2c__ex4__slave_tx_multiple_8c}
\input{usci__b__spi__ex1__master_8c}
\input{usci__b__spi__ex1__slave_8c}
\input{_m_s_p430_f5xx__6xx_2wdt__a_2wdt__a__ex1__interval_s_m_c_l_k_8c}
\input{_m_s_p430_f_r2xx__4xx_2wdt__a_2wdt__a__ex1__interval_s_m_c_l_k_8c}
\input{_m_s_p430_f_r57xx_2wdt__a_2wdt__a__ex1__interval_s_m_c_l_k_8c}
\input{_m_s_p430_f_r5xx__6xx_2wdt__a_2wdt__a__ex1__interval_s_m_c_l_k_8c}
\input{_m_s_p430_f5xx__6xx_2wdt__a_2wdt__a__ex2__interval_a_c_l_k_8c}
\input{_m_s_p430_f_r2xx__4xx_2wdt__a_2wdt__a__ex2__interval_a_c_l_k_8c}
\input{_m_s_p430_f_r57xx_2wdt__a_2wdt__a__ex2__interval_a_c_l_k_8c}
\input{_m_s_p430_f_r5xx__6xx_2wdt__a_2wdt__a__ex2__interval_a_c_l_k_8c}
\input{_m_s_p430_f5xx__6xx_2wdt__a_2wdt__a__ex3__watchdog_a_c_l_k_8c}
\input{_m_s_p430_f_r2xx__4xx_2wdt__a_2wdt__a__ex3__watchdog_a_c_l_k_8c}
\input{_m_s_p430_f_r57xx_2wdt__a_2wdt__a__ex3__watchdog_a_c_l_k_8c}
\input{_m_s_p430_f_r5xx__6xx_2wdt__a_2wdt__a__ex3__watchdog_a_c_l_k_8c}
\input{adc__ex1__avcc_ref_8c}
\input{adc__ex2__int_ref_8c}
\input{_board_8h}
\input{cs__ex1___d_c_o1_m_hz_s_w_trim_8c}
\input{cs__ex2___v_l_o_sources_m_c_l_k_8c}
\input{cs__ex3___x_t1_sources_a_c_l_k_8c}
\input{cs__ex4___x_t_sources_d_c_o_internal_8c}
\input{ecomp__ex1__output_toggle_vcomp_vs_vref1_85_v_8c}
\input{ecomp__ex2__interrupt_vcomp_vs1_85_v_8c}
\input{_m_s_p430_f_r2xx__4xx_2framctl_2framctl__ex1__write_8c}
\input{_m_s_p430_f_r57xx_2framctl_2framctl__ex1__write_8c}
\input{_m_s_p430_f_r5xx__6xx_2framctl_2framctl__ex1__write_8c}
\input{icc__ex1__nested_interrupt_8c}
\input{lcd__e__ex1__4__mux_8c}
\input{_m_s_p430_f_r2xx__4xx_2pmm_2pmm___reset___l_p_mx__5_8c}
\input{_m_s_p430_f_r57xx_2pmm_2pmm___reset___l_p_mx__5_8c}
\input{_m_s_p430_f_r5xx__6xx_2pmm_2pmm___reset___l_p_mx__5_8c}
\input{rtc__ex1__countmode_8c}
\input{sac__ex1__oa_g_p_mode_8c}
\input{sac__ex2__unity_gain_buffer_mode_8c}
\input{sac__ex3__two_stage_amplifier_8c}
\input{sac__ex4__ecomp_8c}
\input{tia__ex1__two_external_inputs_8c}
\input{adc10__b__ex1__avcc_ref_8c}
\input{adc10__b__ex2__int_ref_8c}
\input{comp__d__ex1__output_toggle_vcomp_vs_vref2_v_8c}
\input{comp__d__ex2__output_toggle_vcomp_vs_vref25v_8c}
\input{comp__d__ex3__interrupt_vcomp_vs15_v_8c}
\input{comp__d__ex4__output_toggle_vcomp_vs_half_vcc_8c}
\input{comp__d__ex5__output_toggle_hysteresis_8c}
\input{_m_s_p430_f_r57xx_2cs_2cs__ex1___d_c_o_setup_8c}
\input{_m_s_p430_f_r5xx__6xx_2cs_2cs__ex1___d_c_o_setup_8c}
\input{cs__ex2___d_c_o24_m_hz_8c}
\input{cs__ex3___x_t1_fault_8c}
\input{_m_s_p430_f_r57xx_2mpu_2mpu__ex1__three_seg_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpu_2mpu__ex1__three_seg_8c}
\input{_m_s_p430_f_r57xx_2mpu_2mpu__ex2__two_seg_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpu_2mpu__ex2__two_seg_8c}
\input{_m_s_p430_f_r57xx_2mpu_2mpu__ex3__system_pre_init_8c}
\input{_m_s_p430_f_r5xx__6xx_2mpu_2mpu__ex3__system_pre_init_8c}
\input{ref__ex1__internal_reference_8c}
\input{_m_s_p430_f_r57xx_2rtc__b_2rtc__b__ex1__calendermode_8c}
\input{_m_s_p430_f_r5xx__6xx_2rtc__b_2rtc__b__ex1__calendermode_8c}
\input{adc12__b__ex1__avcc_ref_8c}
\input{adc12__b__ex2__shared_ref_8c}
\input{adc12__b__ex3__ext_ref_8c}
\input{aes256__ex1__encrypt_decrypt_8c}
\input{comp__e__ex1__output_toggle_vcomp_vs_vref2_v_8c}
\input{comp__e__ex2__output_toggle_vcomp_vs_vref25_v_8c}
\input{comp__e__ex3__interrupt_vcomp_vs12_v_8c}
\input{comp__e__ex4__output_toggle_vcomp_vs_half_vcc_8c}
\input{comp__e__ex5__output_toggle_hysteresis_8c}
\input{crc32__ex1__calculate_crc16_8c}
\input{cs__ex2___d_c_o16_m_hz_8c}
\input{framctl__a__ex1__write_8c}
\input{hspll__ex1__output__ussxtosc_8c}
\input{lcd__c__ex1__4mux_8c}
\input{mtif__ex1__pulse_generation_8c}
\input{ram__ex1__set_sector_off_8c}
\input{ref__a__ex1__ctl_a_d_c12_b_8c}
\input{saph__ex1__pulse_generation_8c}
\input{saph__a__ex3__pulse_generation_d_m_a_8c}
\input{sdhs__ex1__8msps__sampling_8c}
\input{cs__ex1__output_clock_signals_8c}
\input{cs__ex2__calculate_clock_signals_8c}
\input{eusci__a__spi__ex1__3_wire_master_8c}
\input{eusci__a__spi__ex1__3_wire_slave_8c}
\input{eusci__a__uart__ex1__loopback115200_baud_8c}
\input{eusci__b__i2c__ex1__master_t_x_multiple_8c}
\input{eusci__b__i2c__ex1__slave_r_x_multiple_8c}
\input{eusci__b__i2c__ex2__master_r_x_multiple_8c}
\input{eusci__b__i2c__ex2__slave_t_x_multiple_8c}
\input{eusci__b__spi__ex1__3_wire_master_8c}
\input{eusci__b__spi__ex1__3_wire_slave_8c}
\input{flashctl__ex1__info_segment_write_8c}
\input{gpio__ex1__toggle_output_8c}
\input{gpio__ex2__input_interrupt_8c}
\input{pmm__ex1__lpm4-5_8c}
\input{pmm__ex2__vmon1160m_v_8c}
\input{sd24__ex1__continuous_conversion_group_channels_8c}
\input{sd24__ex2__single_conversion_group_channels_8c}
\input{sd24__ex3__continuous_conversion_single_channel_8c}
\input{sd24__ex4__single_conversion_single_channel_polling_8c}
\input{sd24__ex5__single_conversion_single_channel_interrupt_8c}
\input{sd24__ex6__single_conversion_single_conversion_temp_sensor_8c}
\input{timer__a__ex1__continuous_overflow_interrupt_8c}
\input{timer__a__ex2__single_p_w_m_8c}
\input{timer__a__ex3__up_mode_interrupt_8c}
\input{timer__a__ex4__period_capture_8c}
\input{tlv__ex1__check_checksum_8c}
\input{wdt__ex1__interval_mode_8c}
\input{wdt__ex2__watchdog_mode_8c}
\input{package_8defs_8h}
\input{package__ti_8mcu_8msp430_8driverlib_8product_8c}
\input{ti__mcu__msp430__driverlib__product_8java}
\input{_9_software_8markdown}
\input{adc10__a_8c}
\input{adc10__a_8h}
\input{adc12__a_8c}
\input{adc12__a_8h}
\input{aes_8c}
\input{aes_8h}
\input{battbak_8c}
\input{battbak_8h}
\input{comp__b_8c}
\input{comp__b_8h}
\input{crc_8c}
\input{crc_8h}
\input{ctsd16_8c}
\input{ctsd16_8h}
\input{dac12__a_8c}
\input{dac12__a_8h}
\input{dma_8c}
\input{dma_8h}
\input{driverlib_8h}
\input{eusci__a__spi_8c}
\input{eusci__a__spi_8h}
\input{eusci__a__uart_8c}
\input{eusci__a__uart_8h}
\input{eusci__b__i2c_8c}
\input{eusci__b__i2c_8h}
\input{eusci__b__spi_8c}
\input{eusci__b__spi_8h}
\input{flashctl_8c}
\input{flashctl_8h}
\input{gpio_8c}
\input{gpio_8h}
\input{hw__memmap_8h}
\input{version_8h}
\input{lcd__b_8c}
\input{lcd__b_8h}
\input{lcd__c_8c}
\input{lcd__c_8h}
\input{ldopwr_8c}
\input{ldopwr_8h}
\input{lextab_8py}
\input{mpy32_8c}
\input{mpy32_8h}
\input{oa_8c}
\input{oa_8h}
\input{pmap_8c}
\input{pmap_8h}
\input{pmm_8c}
\input{pmm_8h}
\input{ram_8c}
\input{ram_8h}
\input{ref_8c}
\input{ref_8h}
\input{rtc__a_8c}
\input{rtc__a_8h}
\input{rtc__b_8c}
\input{rtc__b_8h}
\input{rtc__c_8c}
\input{rtc__c_8h}
\input{sd24__b_8c}
\input{sd24__b_8h}
\input{sfr_8c}
\input{sfr_8h}
\input{sysctl_8c}
\input{sysctl_8h}
\input{tec_8c}
\input{tec_8h}
\input{timer__a_8c}
\input{timer__a_8h}
\input{timer__b_8c}
\input{timer__b_8h}
\input{timer__d_8c}
\input{timer__d_8h}
\input{tlv_8c}
\input{tlv_8h}
\input{ucs_8c}
\input{ucs_8h}
\input{usci__a__spi_8c}
\input{usci__a__spi_8h}
\input{usci__a__uart_8c}
\input{usci__a__uart_8h}
\input{usci__b__i2c_8c}
\input{usci__b__i2c_8h}
\input{usci__b__spi_8c}
\input{usci__b__spi_8h}
\input{wdt__a_8c}
\input{wdt__a_8h}
\input{yacctab_8py}
\input{_software_2_code_01_composer_01_studio_01_workspace_2_sunseeker_telemetry_and_lighting_system_2main_8c}
\input{_resources_2_software_2msp430__driverlib__2__91__13__01_2examples_2_m_s_p430_f5xx__6xx_200__empty_project_2main_8c}
\input{_resources_2_software_2msp430__driverlib__2__91__13__01_2examples_2_m_s_p430_f_r2xx__4xx_200__empty_project_2main_8c}
\input{_resources_2_software_2msp430__driverlib__2__91__13__01_2examples_2_m_s_p430_f_r57xx_200__empty_project_2main_8c}
\input{_resources_2_software_2msp430__driverlib__2__91__13__01_2examples_2_m_s_p430_f_r5xx__6xx_200__empty_project_2main_8c}
\input{_resources_2_software_2msp430__driverlib__2__91__13__01_2examples_2_m_s_p430i2xx_200__empty_project_2main_8c}
%--- End generated contents ---

% Index
\backmatter
\newpage
\phantomsection
\clearemptydoublepage
\addcontentsline{toc}{chapter}{\indexname}
\printindex

\end{document}
