{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":46,"n_cols":4,"rows_kept":46,"flags":["formulas_cached_only"]}
["Displays"]
["LCD Display","Speed, Voltage, Current, Temp.","CAN Bridge Ribbon"]
["LCD Display","4 Programmable, TBD","CAN Bridge Ribbon"]
[]
["Large Switches",null,null,"Switch Type"]
["Enable","Enable CAN HW Elements","DC Conn 12","on-off"]
["Forward-Reverse","Car Direction (on-forward)","DC Conn 13","on-off"]
["Regen Enable","Enable Motor Regen","DC Conn 15","on-off"]
["Hazard Lights","Enable Hazard Light Flash","DC Conn 9","on-off"]
[]
["Turn Signal","Right Turn","DC Conn 7","on-none-on"]
[null,"Left Turn","DC Conn 8"]
[]
["Cruise Control","Rotory Shaft Encoder"]
["CC SW",null,"DC Conn 2"]
["CC Ain",null,"DC Conn 1"]
["CC Bin",null,"DC Conn 20"]
["CC Ground","???","???"]
[]
["Momentary Switches"]
["BPS SW Reset","Reset BPS","BPS SW1","momentary panel"]
["Unknown","??","??","momentary panel"]
[]
[]
[]
[]
["Ground",null,"DC Conn 22, 25-29"]
[]
["Accelerator"]
["Analog 1 Input","Potentiometer Wiper","DC Conn 4"]
["POT Power","Potentiometer +","DC Conn 21"]
["POT Ground","Potentiometer -","DC Conn 22"]
[]
["Small Toggle Switches"]
["MPPT #1","Enable MMPT",null,"on-off"]
["MPPT #2","Enable MMPT",null,"on-off"]
["MPPT #3","Enable MMPT",null,"on-off"]
["MPPT #4","Enable MMPT",null,"on-off"]
["MPPT #5","Enable MMPT",null,"on-off"]
["MPPT #6","Enable MMPT",null,"on-off"]
[]
["Small panel SW","Fan Controls"]
["Driver",null,null,"on-off"]
["Battery",null,null,"on-off"]
["MPPT",null,null,"on-off"]
["Aux","unknown",null,"on-off"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}