{\bfseries{Subpages}} 


\begin{DoxyItemize}
\item \mbox{\hyperlink{deviceSpecifications}{Device Specifications}}
\item \mbox{\hyperlink{layoutPlanning}{Layout Planning}}
\end{DoxyItemize}

\DoxyHorRuler{0}
 \hypertarget{deviceSpecifications}{}\doxysection{Device Specifications}\label{deviceSpecifications}
\hypertarget{device_specifications_autotoc_md1}{}\doxysubsubsection{Microcontroller\+: Texas Instruments MSP430\+F5438\+AIPZR}\label{device_specifications_autotoc_md1}

\begin{DoxyItemize}
\item 1.\+8 V to 3.\+6 V Supply Voltage
\item Capabilities\+:
\begin{DoxyItemize}
\item 16-\/bit architecture
\item 25 MHz System Clock
\end{DoxyItemize}
\item Notable Peripherals\+:
\begin{DoxyItemize}
\item Up to 4 of\+:
\begin{DoxyItemize}
\item UART/\+SPI
\end{DoxyItemize}
\item Up to 4 of\+:
\begin{DoxyItemize}
\item I2\+C/\+SPI
\end{DoxyItemize}
\item 12-\/bit ADC
\begin{DoxyItemize}
\item 14 external channels
\end{DoxyItemize}
\end{DoxyItemize}
\end{DoxyItemize}\hypertarget{device_specifications_autotoc_md2}{}\doxysubsubsection{Real-\/\+Time Clock/\+Calendar\+: Microchip Technology ‎\+MCP7940\+MT-\/\+I/\+SN}\label{device_specifications_autotoc_md2}

\begin{DoxyItemize}
\item 1.\+8 V to 5.\+5 V Supply Voltage
\item Notable Peripherals\+:
\begin{DoxyItemize}
\item I2C
\begin{DoxyItemize}
\item Clock rate up to 400 k\+Hz
\end{DoxyItemize}
\end{DoxyItemize}
\end{DoxyItemize}\hypertarget{device_specifications_autotoc_md3}{}\doxysubsubsection{Bluetooth/\+Wi-\/\+Fi\+: Espressif Systems ESP32-\/\+WROVER-\/\+IE (8\+MB)}\label{device_specifications_autotoc_md3}

\begin{DoxyItemize}
\item 3.\+0 V to 3.\+6 V Supply Voltage
\item Notable Peripherals\+:
\begin{DoxyItemize}
\item I2C
\item SPI
\item UART
\end{DoxyItemize}
\end{DoxyItemize}\hypertarget{device_specifications_autotoc_md4}{}\doxysubsubsection{GPS Receiver\+: Maxim Integrated ‎\+MAX2771\+ETI+T}\label{device_specifications_autotoc_md4}

\begin{DoxyItemize}
\item 2.\+7 V to 3.\+3 V Supply Voltage
\item Notable Peripherals\+:
\begin{DoxyItemize}
\item SPI
\end{DoxyItemize}
\end{DoxyItemize}\hypertarget{device_specifications_autotoc_md5}{}\doxysubsubsection{CANbus Controller\+: Microchip Technology MCP2515\+T-\/\+I/\+SO}\label{device_specifications_autotoc_md5}

\begin{DoxyItemize}
\item 2.\+7 V to 5.\+5 V Supply Voltage
\item Notable Peripherals\+:
\begin{DoxyItemize}
\item SPI
\begin{DoxyItemize}
\item 10 MHz
\end{DoxyItemize}
\end{DoxyItemize}
\end{DoxyItemize}\hypertarget{device_specifications_autotoc_md6}{}\doxysubsubsection{CAN Bus Transceiver\+: ‎\+Microchip Technology MCP2542\+FD-\/\+H/\+SN}\label{device_specifications_autotoc_md6}

\begin{DoxyItemize}
\item 4.\+5 V to 5.\+5 V Supply Voltage
\item Used directly with CANbus Controller
\end{DoxyItemize}\hypertarget{device_specifications_autotoc_md7}{}\doxysubsubsection{SD Card (\+Generic)}\label{device_specifications_autotoc_md7}

\begin{DoxyItemize}
\item 2.\+7 V to 3.\+6 V Supply Voltage
\item Notable Peripherals\+:
\begin{DoxyItemize}
\item SPI
\end{DoxyItemize}
\end{DoxyItemize}\hypertarget{device_specifications_autotoc_md8}{}\doxysubsubsection{USB to UART Bridge\+: FTDI ‎‎\+FT260\+Q-\/T}\label{device_specifications_autotoc_md8}

\begin{DoxyItemize}
\item We will use a \char`\"{}\+Bus-\/\+Powered Configuration\char`\"{}, requiring the host device to supply power, that way we don\textquotesingle{}t have to.
\end{DoxyItemize}\hypertarget{device_specifications_autotoc_md9}{}\doxysubsubsection{RS-\/232 Transceiver\+: Texas Instruments GD75232\+PWR}\label{device_specifications_autotoc_md9}
\hypertarget{device_specifications_autotoc_md10}{}\doxysubsubsection{Inertial Measurement Unit\+: TDK Inven\+Sense ICM-\/20600}\label{device_specifications_autotoc_md10}

\begin{DoxyItemize}
\item 1.\+71 V to 3.\+45 V Supply Voltage
\item Notable Peripherals\+:
\begin{DoxyItemize}
\item I2C
\begin{DoxyItemize}
\item 400 k\+Hz
\end{DoxyItemize}
\item SPI
\begin{DoxyItemize}
\item 10 MHz 
\end{DoxyItemize}
\end{DoxyItemize}
\end{DoxyItemize}\hypertarget{layoutPlanning}{}\doxysection{Layout Planning}\label{layoutPlanning}
\hypertarget{layout_planning_autotoc_md11}{}\doxysubsubsection{Microcontroller}\label{layout_planning_autotoc_md11}
