/*
 * Clock Initialization Code MSP430F5438A
 * Initialize Clock Source XT1 @ 32768 Hz
 * Initialize Clock Source XT2 @ 20MHz
 *
 * Sunseeker Telemetry 2021
 *
 * Last modified October 2015 by Scott Haver
 * Last modified May 2021 by B. Bazuin
 *
 * Main CLK     :  MCLK  = XT2     = 20 MHz
 * Sub-Main CLK :  SMCLK = XT2/2   = 10  MHz
 * Aux CLK      :  ACLK  = XT1     = 32.768 kHz
 *
 */

#ifndef MAIN_H_
#define MAIN_H_

#include <msp430x54xa.h>

#include <stdio.h>


#endif /* MAIN_H_ */
