EESchema-DOCLIB  Version 2.0
#
$CMP 208-8_CTSElectrocomponents
D Dip Switch SPST 8 Position Through Hole Slide (Standard) Actuator 50mA 24VDC
F https://www.ctscorp.com/wp-content/uploads/208.pdf
$ENDCMP
#
$CMP 4116R-1-102LF_Bourns
D 1k Ohm ±2% 250mW Power Per Element Isolated  Resistor Network/Array ±100ppm/°C 16-DIP (0.300", 7.62mm)
F https://www.bourns.com/docs/Product-Datasheets/4100R.pdf
$ENDCMP
#
$CMP 4116R-1-103_Bourns
D 10k Ohm ±2% 250mW Power Per Element Isolated  Resistor Network/Array ±100ppm/°C 16-DIP (0.300", 7.62mm)
F https://www.bourns.com/docs/Product-Datasheets/4100R.pdf
$ENDCMP
#
$CMP 4116R-1-105LF_Bourns
D 1M Ohm ±2% 250mW Power Per Element Isolated  Resistor Network/Array ±100ppm/°C 16-DIP (0.300", 7.62mm)
F https://www.bourns.com/docs/Product-Datasheets/4100R.pdf
$ENDCMP
#
$CMP 4116R-1-331LF_Bourns
D 330 Ohm ±2% 250mW Power Per Element Isolated  Resistor Network/Array ±100ppm/°C 16-DIP (0.300", 7.62mm)
F https://www.bourns.com/docs/Product-Datasheets/4100R.pdf
$ENDCMP
#
$CMP DC10EWA_Kingbright
D LED Circuit Board Indicator Bar - 10 Wide, DIP Red (x 10) Diffused, White 2V 30mA  Through Hole
F http://www.kingbrightusa.com/images/catalog/SPEC/DC10EWA.pdf
$ENDCMP
#
$CMP G5V-2-DC3_OmronElectronics
D General Purpose Relay DPDT (2 Form C) Through Hole
F https://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v_2.pdf
$ENDCMP
#
$CMP NHD-0216BZ-RN-YBW_NewhavenDisplay
D Character LCD Display Module Reflective 5 x 8 Dots STN - Super-Twisted Nematic Without Backlight Parallel 84.00mm x 44.00mm x 9.00mm
F http://www.newhavendisplay.com/specs/NHD-0216BZ-RN-YBW.pdf
$ENDCMP
#
$CMP OS102011MS2QN1_C&K
D Slide Switch SPDT Through Hole
F https://dznh3ojzb2azq.cloudfront.net/products/Slide/OS/documents/datasheet.pdf
$ENDCMP
#
$CMP SN74HCT540N_TexasInstruments
D Buffer, Inverting 1 Element 8 Bit per Element 3-State Output 20-PDIP
F http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fsn74hct540
$ENDCMP
#
$CMP SN74HCT541N_TexasInstruments
D Buffer, Non-Inverting 1 Element 8 Bit per Element 3-State Output 20-PDIP
F http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fsn74hct541
$ENDCMP
#
$CMP SS-13D16-VG_C&K
D Slide Switch SP3T Through Hole
F https://media.digikey.com/pdf/Data%20Sheets/C&K/SS-13D16-VG.pdf
$ENDCMP
#
#End Doc Library
